摄像头第二种模式：摄像头连接路由器模式手机可通过网络观看连接
（只要绑定后，只要摄像头不离开WIFI范围 手机有网络就可无限距离观看使用）
Mode Two: Connect the camera to the router, the phone can watch the connection through the network.
 (As long as the camera keeps being the WIFI range, and the mobile phone has a network, you can watch and use it at any distance.)
1.打开手机设置 open settings

2.	点击进入WLAN连接自己家的无线路由网络 connect your household wifi
3.	打开软件APP open the App
4.	
5.	点击如图位置 click as the picture shows
6.	 5.显示如图界面确认确认A位置应该是自家家的无线路由器ID（选择将要连接的WIFI名称）正确后B位置输入所选择的无线路由器密码都正确后点击NEXT step选项
Confirm that A should be your own router ID; enter the password of the selected wireless router at position B; click the Next Step button.
7.	进入该界面点击如图位置 click as the picture shows

7.	选择连接摄像头的WIFI在确认连接上后进入下一步（该步骤是将设置好的WIFI名称和密码写入到摄像头内使摄像头连接WIFI）注意：该步骤实际是在软件APP内操作而不是在手机自带的设置界面内操作

Choose wifi and confirm connection 
Write the set WIFI name and password into the camera to connect the camera to WIFI. 
Note: This step is actually operated in the software APP.
8.确认连接好后一定要选择如图位置点击返回。（不可以返回手机业主页面再打开APP因为此时的界面是在安装后的APP界面内设置的）

Click to return (Do not directly return back to the phone homepage, cause the interface above is set in the APP interface)

8.	
Confirm the ID is the same as the network ID, otherwise the connection will fail. Click Done.
该步骤需要确认A位置内容是否正确，确认正确后点击B位置选项
Confirm the camera ID; then click Done
9.	确认该位置 连接状态 显示如图选项后 点击该位置进入下一步
Confirm the status and click it to next step
10.	点击后进入既连接完成，此时摄像头已连接无线路由器，确认手机网络状态此时手机网络状态处于连接无线路由器既安装完成。手机也可断开无线网络使用4G使用该APP
Click to enter and the connection is complete. The camera is connected to the wireless router. Confirm the mobile phone network status. The mobile phone network status is connected to the wireless router. The mobile phone can also be disconnected from the wireless network and use 4G.

11.	注：摄像头因没电关机后只要充电完成在WIFI范围内开机后将自动连接不需要重复以上步骤
复位功能：MODE键按住不松开3秒 观察开关键灯（蓝色）会先灭掉然后会快闪后灯会一闪一灭这时机器复位成功，可重新设置连接其他WIFI。

Note: If the camera is turned off due to no power, after the charging is completed, it will automatically connect as long as it is within the WIFI range. There is no need to repeat the above steps.

Reset: Press and hold the MODE button for 3 seconds. The switch key light (blue) will first go out and then flash quickly. When the light keeps flashing, the machine resets successfully, then you can reset it to connect to other WIFI.