G-Index

A B C D E F G H I L M N O P R S T U V W

## G

getAddress(int[]) - Method in class com.ftdi.j2xx.ft4222.FT_4222_I2c_Slave
  Get the address of the I2C slave device.
getAddress(int[]) - Method in interface com.ftdi.j2xx.interfaces.I2cSlave
  Get the address of the I2C slave device.
getBitMode() - Method in class com.ftdi.j2xx.FT_Device
  Gets the instantaneous value of the data bus. Remarks: For a description of available bit modes for the FT232R, see the application note "Bit Bang Modes for the FT232R and FT245R". For a description of available bit modes for the FT2232, see the application note "Bit Mode Functions for the FT2232".
getBufferNumber() - Method in class com.ftdi.j2xx.D2xxManager.DriverParameters
  This method will return Buffer number for Rx in user space application.
getClock(byte[]) - Method in class com.ftdi.j2xx.ft4222.FT_4222_Device
  Get the current system clock rate.
getDeviceInfo() - Method in class com.ftdi.j2xx.FT_Device
  Retrieves information on the device that is currently open.
getDeviceInfoList(int, D2xxManager.FtDeviceInfoListNode[]) - Method in class com.ftdi.j2xx.D2xxManager
  This method returns the device list created with a prior call to `D2xxManager.createDeviceInfoList(Context)`.
getDeviceInfoListDetail(int) - Method in class com.ftdi.j2xx.D2xxManager
  This method returns information for a single device from the internal device list created by a previous call to `D2xxManager.createDeviceInfoList(Context)`.
getEventStatus() - Method in class com.ftdi.j2xx.FT_Device
  This method retrieves the event status
getGpioDevice() - Method in class com.ftdi.j2xx.ft4222.FT_4222_Device
  Get GPIO interface
getI2cMasterDevice() - Method in class com.ftdi.j2xx.ft4222.FT_4222_Device
  Get I2c mater interface
getI2cSlaveDevice() - Method in class com.ftdi.j2xx.ft4222.FT_4222_Device
  Get I2c slave interface
getInstance(Context) - Static method in class com.ftdi.j2xx.D2xxManager
  This method initialises an application, obtaining a value of D2xx device manager.
getLatencyTimer() - Method in class com.ftdi.j2xx.FT_Device
  This method retrieves the current latency timer value from the device.
getLibraryVersion() - Static method in class com.ftdi.j2xx.D2xxManager
  This method returns the D2XX library version number.
getLineStatus() - Method in class com.ftdi.j2xx.FT_Device
  This method retrieves the current modem line status values for the device.
getMaxBufferSize() - Method in class com.ftdi.j2xx.D2xxManager.DriverParameters
  This method will return Rx buffer size of user space application.
getMaxTransferSize() - Method in class com.ftdi.j2xx.D2xxManager.DriverParameters
  This method will return Max Transfer size for Rx in the user space application.
getModemStatus() - Method in class com.ftdi.j2xx.FT_Device
  Retrieves the current modem status values for the device.
getQueueStatus() - Method in class com.ftdi.j2xx.FT_Device
  Retrieves the number of bytes available to read from the driver Rx buffer.
getReadTimeout() - Method in class com.ftdi.j2xx.D2xxManager.DriverParameters
  This method will return timeout values to be used for read operations.
getReadTimeout() - Method in class com.ftdi.j2xx.FT_Device
getResponseCode() - Method in class com.ftdi.j2xx.protocol.SpiSlaveResponseEvent
  Get response code from the event
getRxStatus(int[]) - Method in class com.ftdi.j2xx.ft4222.FT_4222_Spi_Slave
  Get number of bytes in the receive queue.
getRxStatus(int[]) - Method in interface com.ftdi.j2xx.interfaces.SpiSlave
  Get number of bytes in the receive queue.
getSpiMasterDevice() - Method in class com.ftdi.j2xx.ft4222.FT_4222_Device
  Get Spi mater interface
getSpiSlaveDevice() - Method in class com.ftdi.j2xx.ft4222.FT_4222_Device
  Get Spi slave interface
getStatus(int, byte[]) - Method in class com.ftdi.j2xx.ft4222.FT_4222_I2c_Master
  Read the status of the I2C master controller.
getStatus(int, byte[]) - Method in interface com.ftdi.j2xx.interfaces.I2cMaster
  Read the status of the I2C master controller.
getVIDPID() - Method in class com.ftdi.j2xx.D2xxManager
  This retrieves the current VID and PID combination from within the internal device list table.
Gpio - Interface in com.ftdi.j2xx.interfaces
GPIO_INPUT - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.GPIO_Dir
GPIO_OUTPUT - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.GPIO_Dir
GPIO_OUTPUT_HIGH - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.GPIO_Output
GPIO_OUTPUT_LOW - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.GPIO_Output
GPIO_PORT0 - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.GPIO_Port
GPIO_PORT1 - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.GPIO_Port
GPIO_PORT2 - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.GPIO_Port
GPIO_PORT3 - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.GPIO_Port
GPIO_TRIGGER_FALLING - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.GPIO_Tigger
GPIO_TRIGGER_LEVEL_HIGH - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.GPIO_Tigger
GPIO_TRIGGER_LEVEL_LOW - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.GPIO_Tigger
GPIO_TRIGGER_RISING - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.GPIO_Tigger

A B C D E F G H I L M N O P R S T U V W

About FTDI | FTDI Licence Terms