Output of 'file' command:
=========================
./build/arm-v7-hf/libftd2xx.so.1.4.6: ELF 32-bit LSB  shared object, ARM, EABI5 version 1 (SYSV), dynamically linked, BuildID[sha1]=3195183007e166a5edf9b05268af4f9475e3dded, not stripped
Output of 'readelf -A' command:
===============================
Attribute Section: aeabi
File Attributes
  Tag_CPU_name: "7-A"
  Tag_CPU_arch: v7
  Tag_CPU_arch_profile: Application
  Tag_ARM_ISA_use: Yes
  Tag_THUMB_ISA_use: Thumb-2
  Tag_FP_arch: VFPv3-D16
  Tag_ABI_PCS_wchar_t: 4
  Tag_ABI_FP_rounding: Needed
  Tag_ABI_FP_denormal: Needed
  Tag_ABI_FP_exceptions: Needed
  Tag_ABI_FP_number_model: IEEE 754
  Tag_ABI_align_needed: 8-byte
  Tag_ABI_align_preserved: 8-byte, except leaf SP
  Tag_ABI_enum_size: int
  Tag_ABI_HardFP_use: SP and DP
  Tag_ABI_VFP_args: VFP registers
  Tag_CPU_unaligned_access: v6
