Quad SDI Capture Card Driver Installation Instruction

1. Insert the capture card into the PCIe slot of the computer motherboard, and turn on the computer.

2. Enter the computer management---->Device Manager----->other devices (multimedia video controller), and find the new device.

3. Open the folder where the driver is located, choose 64-bit or 32-bit driver according to the operating system, click Install, a driver installation dialog box will pop up (showing that a capture card is found), and you can install it!

